**Powder Touch-Up Pens**

Repair pen for refurbishing powder paint in all colours

**Description**

* Metal screw top can, filled with 12ml transparent basic enamel paint, brush and washer (in PVC)
* White plastic measuring cup for required colour powder

**Use**

1. Pull the screw top with brush and washer (PVC) out of the metal can by turning clockwise. (Do not unscrew)

i.e. remove the entire plastic assembly from the metal can.

1. Place the desired colour powder in the measuring cup: approx. ¾ full.
2. Then add the powder to the solvent in the metal can and stir with the brush.
3. Then replace screw to p and washer (entire plastic assembly) in the metal can (press).
4. Shake vigorously (approx. 1 min.) so that you can hear the ball in the can.
5. Apply the enamel paint in thin layers.

**Drying Time**

Approx. 20 minutes

**Storage Stability**

* Unmixed (separately) : 2 to 3 years, dry and frost-proof
* Mixed : approx. 3 days when the can is properly closed

**Packaging**

Pack of 1 or 10 pens of 12 ml.